WHEEL AND TIRE SPECIFICATION

id021200800100

Wheel and tire

Item | Specification
--- | ---
Standard tire and wheel
Wheel | Size | 16 × 6 1/2JJ | 16 × 6 1/2J | 17 × 7J
Offset | (mm {in}) | 50 {2.0} | 55 {2.17}
Pitch circle diameter | (mm {in}) | 114.3 {4.50}
Material | Steel | Aluminum alloy
Tire | Size | 205/50R16 87V | 205/45R17 84W
Air pressure (kPa {kgf/cm2, psi}) | Front | 200 {2.0, 29}
Rear | 200 {2.0, 29}
Remaining tread | (mm {in}) | 1.6 {0.06}
Wheel and tire | Wheel and tire runout | Radial direction | 1.5 {0.06} max.
(mm {in}) | Lateral direction | 2.5 {0.10} max. | 2.0 {0.08} max.
Wheel imbalance | (g {oz}) | 9 {0.3} max. | Adhesive-type*1: 14 {0.49} max. Knock-type*2: 9 {0.3} max | Adhesive-type*1: 13 {0.46} max Knock-type*2: 8 {0.28} max

*1 :Total weight exceeds 160 g {5.65 oz}.
*2 :One balance weight: 60 g {2.12 oz} max. If the total weight exceeds 100 g {3.53 oz} on one side, rebalance after moving the tire around on the rim. Do not use three or more balance weights.