BACK-UP LIGHT SWITCH REMOVAL/INSTALLATION [P66M-D]

id051111248000

1. Remove the battery cover.

2. Disconnect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

3. Loosen the starter installation bolts only enough that the starter is loose, but not removed. (See STARTER REMOVAL/INSTALLATION [L8, LF].)

4. Remove the transmission. (See TRANSMISSION REMOVAL/INSTALLATION [P66M-D].)

5. Disconnect the back-up light switch connector and remove the back-up light switch.

amxzzw00001878

6. Install the back-up light switch (with a new gasket) to the transaxle case.

  Tightening torque

  25—34 N·m {2.5—3.5 kgf·m, 18—25 ft·lbf}

7. Install in the reverse order of removal.