AIRFLOW MODE CONTROL OPERATION [FULL-AUTO AIR CONDITIONER]

id0740a1102900

Airflow Mode Automatic Control

• The climate control unit calculates the mode actuator opening angle (airflow mode) based on the target temperature operating the actuator.

amxzzn00000355

Correction

MAX HOT and MAX COLD correction
• When the set temperature is at 29, the airflow mode is set to HEAT, when it is at 15, it is set to vent.

Airflow Mode Manual Control

• The airflow mode can be switched by operating the airflow mode dial.