HEADLIGHT BULB REMOVAL/INSTALLATION

id091800464100

Low-beam

Halogen type

1. Remove the battery cover.

2. Disconnect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

3. Remove the fasteners, then slightly bend back the mudguard.

4. Disconnect the connector.

amxzzw00001883

  Caution
  • A halogen bulb generates extremely high heat when it is illuminated. If the surface of the bulb is soiled, excessive heat will build up and the life of the bulb will be shortened. When replacing the bulb, hold the metal flange, not the glass.

5. Remove the cover.

6. Remove the socket, then remove the headlight bulb.

7. Install in the reverse order of removal.

Discharge type

  Warning
  • Incorrect servicing of the discharge headlights could result in electrical shock. Before servicing the discharge headlights, always refer to the discharge headlight service warnings. (See DISCHARGE HEADLIGHT SERVICE WARNINGS.)

1. Remove the battery cover.

2. Disconnect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

3. Remove the fasteners, then slightly bend back the mudguard.

4. Remove the cover.

amxzzw00001884

  Caution
  • The discharge headlight generates extremely high heat when it is illuminated. If the surface of the discharge headlight is soiled, excessive heat will build up and the life of the discharge headlight will be shortened. When replacing the bulb, hold the metal flange, not the glass.

5. Remove the discharge connector. (See Discharge connector removal note.)

6. Remove the discharge headlight (See Discharge headlight removal note.)

7. Install in the reverse order of removal.

Discharge connector removal note

1. Rotate the discharge connector in the direction of the arrow shown in the figure to remove it.

amxzzw00001885

Discharge headlight removal note

1. Press sections A to release the bulb retaining wire and remove the discharge headlight.

amxzzw00001041

High-beam

1. Remove the battery cover.

2. Disconnect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

3. Disconnect the connector.

amxzzw00001039

  Caution
  • A halogen bulb generates extremely high heat when it is illuminated. If the surface of the bulb is soiled, excessive heat will build up and the life of the bulb will be shortened. When replacing the bulb, hold the metal flange, not the glass.

4. Remove the socket, then remove the headlight bulb.

5. Install in the reverse order of removal.