SIDE SILL REINFORCEMENT INSTALLATION [PANEL REPLACEMENT]

id098008609300

  Caution
  • The side sill reinforcement installation procedure is based on the condition that the cowl side panel and the hinge pillar (outer) and the rear fender panel have been removed.

1. When installing new parts, measure and adjust the body as necessary to conform with standard dimensions.

2. Drill holes for plug welds before installing new parts.

3. After temporarily installing new parts, make sure the related parts fit properly.

d5u0980b090