POWER OUTER MIRROR INSPECTION

id091200803000

1. Apply battery positive voltage and connect the ground to the corresponding power outer mirror terminals, and then inspect the operation of the power outer mirror.

amxzzw00000717

  • If not as specified, replace the power outer mirror.

Operation | Terminal
--- | ---
B+ | GND
Up | B | D
Down | D | B
Left | F | D
Right | D | F

2. Inspect for continuity between the power outer mirror heater terminals.

amxzzw00000718

  • If not as specified, replace the power outer mirror.

amxzzw00000719