CYLINDER HEAD INSPECTION

id011000507100

1. Perform color contrast penetrate examination on the cylinder head surface.

  • Replace the cylinder head if necessary.

2. Inspect for the following and repair or replace if necessary.

  (1) Sunken valve seats

  (2) Excessive camshaft oil clearance and end play

3. Measure the cylinder head for distortion in six directions as shown in the figure.

  • If it exceeds the maximum specification, replace the cylinder head. Do not attempt to repair the cylinder head by milling or grinding.

belbze00000220

  Maximum distortion:

  0.10 mm {0.004 in}

4. Measure the manifold contact surface distortion as shown in the figure.

  • If it exceeds the maximum specification, grind the surface or replace the cylinder head.

belbze00000221

  Maximum distortion:

  0.10 mm {0.004 in}

  Maximum grinding:

  0.15 mm {0.006 in}