TIMING CHAIN DISASSEMBLY

id011000505500

1. Disassemble in the order indicated in the table.

belbze00000176

1 | Dipstick (If equipped)
2 | Spark plug
3 | Cylinder head cover
4 | Crankshaft pulley lock bolt (See Crankshaft Pulley Lock Bolt Disassembly Note.)
5 | Crankshaft pulley
6 | Water pump pulley
7 | Drive belt idler pulley (If equipped)
8 | Engine front cover
9 | Front oil seal (See Front Oil Seal Disassembly Note.)
10 | Chain tensioner (See Chain Tensioner Disassembly Note.)
11 | Tensioner arm
12 | Chain guide
13 | Timing chain
14 | Seal (If equipped)
15 | Oil pump chain tensioner
16 | Oil pump chain guide (If equipped)
17 | Oil pump sprocket (See Oil Pump Sprocket Disassembly Note.)
18 | Oil pump chain
19 | Crankshaft sprocket

Crankshaft Pulley Lock Bolt Disassembly Note

1. Install the SST to the ring gear to lock the crankshaft against rotation.

belbze00000034

Front Oil Seal Disassembly Note

1. Remove the oil seal using a flat head screwdriver.

belbze00000035

Chain Tensioner Disassembly Note

1. Hold the chain tensioner ratchet lock mechanism away from the ratchet stem with a thin screwdriver.

2. Slowly press the tensioner piston.

3. Hold the chain tensioner piston with a 1.5 mm {0.06 in}wire or paper clip.

belbze00000036

Oil Pump Sprocket Disassembly Note

1. Temporarily install the crankshaft pulley and crankshaft pulley lock bolt to the crankshaft, and lock the oil pump against rotation as shown in figure.

belbze00000037

2. Remove the oil pump sprocket, and then remove the crankshaft pulley and crankshaft pulley lock bolt.