POWER RETRACTABLE HARDTOP SYSTEM OUTLINE

id091600101000

• A switch-operated, open/close power retractable hardtop system has been adopted.
• The power retractable hardtop system consists of the following functions:

  ― Auto-open/close function
  ― Fail-safe function
  ― Malfunction detection function

• The buzzer sounds during operation and when a malfunction is detected.
• Since the power retractable hardtop operates in conjunction with the power windows, the door glass opens 100 mm at the same time the power retractable hardtop begins to operate.