DTC P0108 [L8, LF]

id0102b1803500

DTC P0108 | MAP sensor circuit high input
--- | ---
DETECTION CONDITION | • The PCM monitors the input voltage from the MAP sensor when intake air temperature is above –10 °C {14 °F}. If input the voltage is above 4.92 V, the PCM determines that the MAP sensor circuit has a malfunction. MONITORING CONDITIONS ― Calculated load: 13—32% Diagnostic support note • This is a continuous monitor (CCM). • The MIL illuminates if the PCM detects the above malfunction condition during first drive cycle. • FREEZE FRAME DATA (Mode 2/Mode 12) is available. • The DTC is stored in the PCM memory.
POSSIBLE CAUSE | • MAP sensor connector or terminals malfunction • PCM connector or terminals malfunction • Short to power supply in wiring harness between MAP sensor terminal D and PCM terminal 2AG • MAP sensor power supply circuit and signal circuit are shorted to each other • Open circuit in wiring harness between the following terminals: ― MAP sensor terminal D and PCM terminal 2AG ― MAP sensor terminal A and PCM terminal 2AV • MAP sensor malfunction • PCM malfunction

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | VERIFY FREEZE FRAME DATA (MODE 12) HAS BEEN RECORDED • Has the FREEZE FRAME DATA (Mode 12) been recorded? | Yes | Go to the next step.
No | Record the FREEZE FRAME DATA (Mode 12) on the repair order, then go to the next step.
2 | VERIFY RELATED SERVICE INFORMATION AVAILABILITY • Verify related Service Information availability. • Is any related Service Information available? | Yes | Perform repair or diagnosis according to the available Service Information. • If the vehicle is not repaired, go to the next step.
No | Go to the next step.
3 | INSPECT MAP SENSOR CONNECTOR AND TERMINALS • Turn the ignition switch off. • Disconnect the MAP sensor connector. • Inspect for poor connection (such as damaged/pulled-out pins, corrosion). • Is there any malfunction? | Yes | Repair or replace the connector or terminals, then go to Step 9.
No | Go to the next step.
4 | INSPECT PCM CONNECTOR AND TERMINALS • Disconnect the PCM connector. • Inspect for poor connection at terminals (such as damaged/pulled-out pins, corrosion). • Is there any malfunction? | Yes | Repair or replace the connector or terminals, then go to Step 9.
No | Go to the next step.
5 | INSPECT MAP SENSOR SIGNAL CIRCUIT FOR SHORT TO POWER SUPPLY • MAP sensor and PCM connectors are disconnected. • Turn the ignition switch to the ON position (engine off). • Measure the voltage between the MAP sensor terminal D (wiring harness-side) and body ground. • Is there any voltage? | Yes | Repair or replace the wiring harness for a possible short to power supply, then go to Step 9.
No | Go to the next step.
6 | INSPECT MAP SENSOR POWER SUPPLY AND SIGNAL CIRCUIT FOR SHORT TO EACH OTHER • MAP sensor and PCM connectors are disconnected. • Turn the ignition switch off. • Inspect for continuity between MAP sensor terminal D and C (wiring harness-side). • Is there continuity? | Yes | Repair or replace the suspected wiring harness, then go to Step 9.
No | Go to the next step.
7 | INSPECT MAP SENSOR CIRCUIT FOR OPEN CIRCUIT • MAP sensor and PCM connectors are disconnected. • Inspect for continuity between the following terminals (wiring harness-side): ― MAP sensor terminal D and PCM terminal 2AG ― MAP sensor terminal A and PCM terminal 2AV • Is there continuity? | Yes | Go to the next step.
No | Repair or replace the wiring harness for a possible open circuit, then go to Step 9.
8 | INSPECT MAP SENSOR • Reconnect the MAP sensor connector. • Inspect the MAP sensor. (See MANIFOLD ABSOLUTE PRESSURE (MAP) SENSOR INSPECTION [L8, LF].) • Is there any malfunction? | Yes | Replace the MAP sensor, then go to the next step. (See MANIFOLD ABSOLUTE PRESSURE (MAP) SENSOR REMOVAL/INSTALLATION [L8, LF].)
No | Go to the next step.
9 | VERIFY DTC TROUBLESHOOTING COMPLETED • Make sure to reconnect all disconnected connectors. • Turn the ignition switch to the ON position (engine off). • Clear the DTC from the PCM memory using the M-MDS. (See AFTER REPAIR PROCEDURE [L8, LF].) • Start the engine and warm it up completely. • Perform the KOEO/KOER self test. (See KOEO/KOER SELF TEST [L8, LF].) • Is the same DTC present? | Yes | Replace the PCM, then go to the next step. (See PCM REMOVAL/INSTALLATION [L8, LF].)
No | Go to the next step.
10 | VERIFY AFTER REPAIR PROCEDURE • Perform the “AFTER REPAIR PROCEDURE”. (See AFTER REPAIR PROCEDURE [L8, LF].) • Are any DTCs present? | Yes | Go to the applicable DTC troubleshooting. (See DTC TABLE [L8, LF].)
No | DTC troubleshooting completed.