MANIFOLD ABSOLUTE PRESSURE (MAP) SENSOR REMOVAL/INSTALLATION [L8, LF]

id0140i7804300

1. Remove the battery cover. (See BATTERY REMOVAL/INSTALLATION [L8, LF])

2. Disconnect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION [L8, LF])

3. Remove the dynamic chamber. (See INTAKE-AIR SYSTEM REMOVAL/INSTALLATION [L8, LF].)

4. Remove the MAP sensor.

e5u140zw5k03

5. Install in the reverse order of removal.

  MAP sensor tightening torque

  2.7—3.7 N·m {28—37 kgf·cm, 24—32 in·lbf}