FRONT ROOF PANEL DISASSEMBLY/ASSEMBLY

id091600810800

1. Disassemble in the order indicated in the table.

2. Assemble in the reverse order of disassembly.

e5e916zw6052

1 | Top lock lever cover
2 | Top lock cover
3 | Roof hook wedge
4 | Top lock
5 | Male wedge cover
6 | Male wedge
7 | Weatherstrip
8 | Retainer (See Retainer Disassembly Note.) (See Retainer Assembly Note.)
9 | Front roof panel

Retainer Disassembly Note

1. Mark around the retainer installation screws with paint before removing them.

e5e916zw6053

Retainer Assembly Note

1. Install the retainers to the link, aligning the retainer marks with the retainer installation screws.

e5e916zw6053