BRAKE SYSTEM/ABS WARNING LIGHT CONSTRUCTION/OPERATION

id041300200200

• When the ABS and CAN lines are functioning normally, the brake system/ABS warning light illuminates when the ignition is switched to ON to check for a burned-out bulb, and then turns off after Approx. 3 s. At this time, while the parking brake is activated, the brake system warning light remains illuminated, however, it turns off after the parking brake is released.
• The brake system/ABS warning light illuminates during a system malfunction, and the control is as follows:

Brake system warning light illuminated:
  ― EBD control disabled.

ABS warning light illuminated:
  ― ABS control disabled.

• When the brake switch is malfunctioning, the brake system warning light illuminates but the ABS and EBD controls are not inhibited. (Applied VIN (assumed): NC18**215550—, NC18**250831—, NC30**202488—, NCA8**251024— (vehicles without malfunction warning light))

amxzzn00000489