ACCESSORY SOCKET REMOVAL/INSTALLATION

id092000800400

1. Remove the battery cover.

2. Disconnect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

3. Remove the console. (See CONSOLE REMOVAL/INSTALLATION.)

4. Remove the side wall. (See SIDE WALL REMOVAL/INSTALLATION.)

5. Remove the console panel. (See CONSOLE PANEL REMOVAL/INSTALLATION.)

6. Remove in the order indicated in the table.

amxzzw00001662

1 | Accessory socket (See Accessory Socket Removal Note.)
2 | Cap (See Cap Removal Note.)

7. Install in the reverse order of removal.

Accessory Socket Removal Note

1. While pressing a tape-wrapped fastener remover against the cap projection, pull the accessory socket outward.

e5u920zw5105

Cap Removal Note

1. While pressing the tabs, pull the cap outwards.

amxzzw00001663