POWER WINDOW REGULATOR REMOVAL/INSTALLATION

id091200812700

1. Remove the battery cover.

2. Disconnect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

3. Remove the door trim. (See DOOR TRIM REMOVAL/INSTALLATION.)

4. Remove the door module panel. (See DOOR MODULE PANEL REMOVAL/INSTALLATION.)

5. Remove the door glass. (See DOOR GLASS REMOVAL/INSTALLATION.)

6. Remove the nuts.

e5u912zw5007

7. Remove the power window regulator.

e5u912zw5008

8. Install in the reverse order of removal.