POWERFLOW OPERATION [SJ6A-EL]

id051311320600

List of operating components

Clutch/Brake | Operation
--- | ---
C1 clutch | • Engages input shaft and intermediate shaft via F4 one-way clutch.
C2 clutch | • Engages input shaft and middle planetary carrier.
C3 clutch | • Engages input shaft and front sun gear.
C4 clutch | • Engages input shaft and intermediate shaft.
B1 brake | • Locks rotation of front planetary carrier.
B2 brake | • Locks rotation of front and middle ring gear.
B3 brake | • Locks F2 one-way clutch outer race.
B4 brake | • Locks rotation of rear ring gear.
F1 one-way clutch | • Locks counterclockwise rotation of front planetary carrier on transmission case.
F2 one-way clutch | • Locks counterclockwise rotation of front sun gear during B3 brake operation.
F3 one-way clutch | • Locks counterclockwise rotation of rear ring gear. • Locks counterclockwise rotation of middle planetary carrier.
F4 one-way clutch | • Locks counterclockwise rotation of intermediate shaft during C1 clutch operation.

1GR

ar8wzn00000041

ar8wzn00000042

2GR

ar8wzn00000043

ar8wzn00000044

3GR

ar8wzn00000045

ar8wzn00000046

4GR

ar8wzn00000047

ar8wzn00000048

5GR

ar8wzn00000049

ar8wzn00000050

6GR

ar8wzn00000051

ar8wzn00000052

R position

ar8wzn00000053

ar8wzn00000054