VARIABLE INTAKE AIR SOLENOID VALVE INSPECTION [L8, LF]

id0113a3802800

Airflow Inspection

1. Remove the battery cover. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

2. Disconnect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

3. Remove the variable intake air solenoid valve. (See VARIABLE INTAKE AIR SOLENOID VALVE REMOVAL/INSTALLATION [L8, LF].)

4. Inspect airflow between the ports under the following conditions.

amxzzw00000900

amxzzw00000801

  • If not as specified, replace the variable intake air solenoid valve. (See VARIABLE INTAKE AIR SOLENOID VALVE REMOVAL/INSTALLATION [L8, LF].)