DLC-2 OUTLINE [SJ6A-EL]

id050208100900

• A connector (DLC-2) conforming to International Organization for Standardization (ISO) standards has been added.
• Shape and terminal arrangement as stipulated by the ISO 15031-3 (SAE J1962) international standard has been adopted for this connector. The connector has a 16-pin construction that includes the B+, CAN_H, CAN_L, GND1, GND2 and KLN terminals.

amxzzn00000079

Terminal | Function
--- | ---
B+ | Battery power supply terminal
CAN_L | Serial communication Lo terminal
CAN_H | Serial communication Hi terminal
GND1 | Body ground terminal
GND2 | Serial communication ground terminal
KLN | Serial communication terminal (malfunction diagnosis use)