CRUSHABLE ZONE CONSTRUCTION

id091000100400

• High-tensile-strength plates with an octagonal profile are used for the front bumper reinforcement and front side frames have been placed to absorb the impact force of a frontal collision.

e5u910zs1004

• A three-pronged structure, capable of dispersing impact force received by the front side frame in three directions, has been adopted. It also suppresses cabin deformation in offset frontal collisions.

e5u910zs1001