BLACK-OUT FILM REMOVAL

id091600821500

Front

1. Partially peel back the middle roof weatherstrip.

2. Peel off the black-out film by pulling it outward from one end.

amxzzw00001920

  Note
  • Slowly remove the black-out film since it may tear easily.

Rear

1. Move the power retractable hardtop in the open direction as shown in the figure until it is separated from the middle roof panel.

amxzzw00001921

2. Peel off the black-out film by pulling it outward from one end.

amxzzw00002325

  Note
  • Slowly remove the black-out film since it may tear easily.