DTC TABLE [ACTIVE BONNET]

id0802f1080700

X: Applicable
−: Not applicable

DTC | Active bonnet warning light | System malfunction location | Memory function | Reference
--- | --- | --- | --- | ---
Flashing pattern | Order of precedence
B00D2:01 | − | Continuously illuminated | 1 | Active bonnet warning light malfunction | X | (See DTC B00D2:01 [ACTIVE BONNET].)
B00D2:29 | Active bonnet warning light communication error | X | (See DTC B00D2:29 [ACTIVE BONNET].)
B1001:11 | 19 |  | 11 | Active bonnet actuator (RH) circuit short to ground | X | (See DTC B1001:11/B1001:12/B1001:13/B1001:19/B1001:1A [ACTIVE BONNET].)
B1001:12 | Active bonnet actuator (RH) circuit short to power supply | X
B1001:13 | Active bonnet actuator (RH) circuit open circuit or resistance high | X
B1001:19 | Short circuit in active bonnet actuator (RH) and (LH) circuits | X
B1001:1A | Active bonnet actuator (RH) circuit resistance low | X
B1003:11 | 21 |  | 10 | Active bonnet actuator (LH) circuit short to ground | X | (See DTC B1003:11/B1003:12/B1003:13/B1003:19/B1003:1A [ACTIVE BONNET].)
B1003:12 | Active bonnet actuator (LH) circuit short to power supply | X
B1003:13 | Active bonnet actuator (LH) circuit open circuit or resistance high | X
B1003:19 | Short circuit in active bonnet actuator (LH) and (RH) circuits | X
B1003:1A | Active bonnet actuator (LH) circuit resistance low | X
B1011:95 | 58 |  | 5 | Active bonnet control module connector partially disconnected | X | (See DTC B1011:95 [ACTIVE BONNET].)
B1193:00 | 13 |  | 3 | Recording of active bonnet control module collision data | X | (See DTC B1193:00 [ACTIVE BONNET].)
B1422:11 | 44 |  | 6 | Active bonnet sensor (right) circuit short to ground | X | (See DTC B1422:11/B1422:13/B1422:87 [ACTIVE BONNET].)
B1422:13 | Active bonnet sensor (right) circuit open circuit or short to body ground | X
B1422:87 | No reception of active bonnet sensor (right) signal | X
B1422:55 | Active bonnet control module internal malfunction | X | (See DTC B1422:55 [ACTIVE BONNET].)
B1422:96 | Active bonnet sensor (right) internal malfunction | X | (See DTC B1422:96 [ACTIVE BONNET].)
B1423:11 | 43 |  | 7 | Active bonnet sensor (right, center) circuit short to ground | X | (See DTC B1423:11/B1423:13/B1423:87 [ACTIVE BONNET].)
B1423:13 | Active bonnet sensor (right, center) circuit open circuit or short to power supply | X
B1423:87 | No reception of active bonnet sensor (right, center) signal | X
B1423:55 | Active bonnet control module internal malfunction | X | (See DTC B1423:55 [ACTIVE BONNET].)
B1423:96 | Active bonnet sensor (right, center) internal malfunction | X | (See DTC B1423:96 [ACTIVE BONNET].)
B1424:11 | 46 |  | 8 | Active bonnet sensor (left, center) circuit short to ground | X | (See DTC B1424:11/B1424:13/B1424:87 [ACTIVE BONNET].)
B1424:13 | Active bonnet sensor (left, center) circuit open circuit or short to power supply | X
B1424:87 | No reception of active bonnet sensor (left, center) signal | X
B1424:55 | Active bonnet control module internal malfunction | X | (See DTC B1424:55 [ACTIVE BONNET].)
B1424:96 | Active bonnet sensor (left, center) internal malfunction | X | (See DTC B1424:96 [ACTIVE BONNET].)
B1425:11 | 45 |  | 9 | Active bonnet sensor (left) circuit short to ground | X | (See DTC B1425:11/B1425:13/B1425:87 [ACTIVE BONNET].)
B1425:13 | Active bonnet sensor (left) circuit open circuit or short to power supply | X
B1425:87 | No reception of active bonnet sensor (left) signal | X
B1425:55 | Active bonnet control module internal malfunction | X | (See DTC B1425:55 [ACTIVE BONNET].)
B1425:96 | Active bonnet sensor (left) internal malfunction | X | (See DTC B1425:96 [ACTIVE BONNET].)
U0001:88 | 14 |  | 4 | CAN communication error | X | (See FOREWORD [MULTIPLEX COMMUNICATION SYSTEM (L.H.D.)].) (See FOREWORD [MULTIPLEX COMMUNICATION SYSTEM (R.H.D.)].)
U0100:68 | Communication error with PCM (vehicle speed signal) | X | (See DTC U0100:68 [ACTIVE BONNET].)
U0155:00 | Instrument cluster communication error | X | (See FOREWORD [MULTIPLEX COMMUNICATION SYSTEM (L.H.D.)].) (See FOREWORD [MULTIPLEX COMMUNICATION SYSTEM (R.H.D.)].)
U3000:49 | 12 |  | 2 | Active bonnet control module internal malfunction | X | (See DTC U3000:49 [ACTIVE BONNET].)
U3003:16 | − | Continuously illuminated | 1 | Active bonnet control module power supply voltage decrease (less than 8 V) | X | (See DTC U3003:16/U3003:17 [ACTIVE BONNET].)
U3003:17 | Active bonnet control module power supply voltage increase (18 V or more) | X