BONNET LATCH SWITCH INSPECTION

id091400810500

1. Open the bonnet.

2. Disconnect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

3. Disconnect the bonnet latch switch connector.

4. Inspect for continuity between the bonnet latch switch terminals A and B.

amxzzw00002135

  • If there is no continuity, replace the bonnet latch switch.

5. Lock the bonnet latch using a flathead screwdriver or equivalent as shown.

amxzzw00002136

6. Inspect for continuity between the bonnet latch switch terminals A and B

  • If there is continuity, replace the bonnet latch.

  Caution
  • After the inspection, unlock the bonnet latch. If closing the bonnet with the bonnet latch locked, the bonnet latch and/or bonnet striker may be broken.