B1, B3 BRAKE AND F1, F2 ONE-WAY CLUTCH COMPONENT ASSEMBLY

id051300261100

Components

bsj6za00000625

1 | B1 brake cylinder
2 | O-ring
3 | B1 brake piston
4 | Spring return
5 | Snap ring
6 | Driven plate
7 | Drive plate
8 | Retaining plate
9 | Bearing race
10 | Thrust washer
11 | F1 one-way clutch
12 | B3 brake cylinder
13 | O-ring
14 | B3 brake cylinder
15 | Piston return spring
16 | Snap ring
17 | Driven plate
18 | Drive plate
19 | Driven plate
20 | Snap ring
21 | Thrust washer
22 | F2 one-way clutch
23 | Thrust washer

Assembly Procedure

1. Apply ATF to the new O-rings.

2. Install the O-rings to the B1 brake piston.

bsj6za00000252

3. Apply ATF to the B1 brake piston and the B1 brake cylinder.

  Caution
  • Do not damage the O-ring.

4. Install the B1 brake piston to the B1 brake cylinder.

bsj6za00000253

5. Apply ATF to the new O-rings.

6. Install the O-rings to the B3 brake piston.

bsj6za00000254

7. Apply ATF to the B3 brake cylinder to the B3 brake piston.

  Caution
  • Do not damage the O-ring.

8. Install the B3 brake piston to the B3 brake cylinder.

bsj6za00000255

9. Install the piston return spring to the B3 brake piston.

bsj6za00000256

10. While holding the snap ring with a finger, install it to the brake cylinder using a flathead screwdriver.

bsj6za00000785

11. Apply ATF to the thrust washer.

12. Install the bearing race to the thrust washer.

13. Install the F1 one-way clutch to the bearing race.

bsj6za00000258

14. Install the B3 brake cylinder to the F1 one-way clutch.

bsj6za00000259