#
WHEEL HUB, STEERING KNUCKLE REMOVAL/INSTALLATION

id031100800400

  Caution

  • Performing the following procedures without first removing the ABS wheel-speed sensor may possibly cause an open circuit in the wiring harness if it is pulled by mistake. Before performing the following procedures, remove the ABS wheel-speed sensor (axle side) and fix it to an appropriate place where the sensor will not be pulled by mistake while servicing the vehicle.

  Note

  • When disassembling/assembling the steering knuckle, remove the two hub bolts diagonally in advance. (See WHEEL HUB BOLT REPLACEMENT.)

1. Remove the ABS wheel-speed sensor. (See FRONT ABS WHEEL-SPEED SENSOR REMOVAL/INSTALLATION.)

2. Remove in the order indicated in the table.

3. Install in the reverse order of removal.

4. After installation, inspect the front wheel alignment.

(See FRONT WHEEL ALIGNMENT.)

.

1 | Locknut
2 | Brake caliper component (See Brake Caliper Component Removal Note.)
3 | Disc plate (See FRONT BRAKE (DISC) REMOVAL/INSTALLATION.)
4 | Tie-rod end (See STEERING GEAR AND LINKAGE REMOVAL/INSTALLATION.)
5 | Front lower arm ball joint
6 | Stabilizer control link (upper side)
7 | Wheel hub, steering knuckle component (See Wheel Hub, Steering Knuckle Component Removal Note.) (See Wheel Hub, Steering Knuckle Component Installation Note.)

## Brake Caliper Component Removal Note

1. Remove the brake caliper component, and suspend it using wire.

## Wheel Hub, Steering Knuckle Component Removal Note

1. Separate the shock absorber and wheel hub/steering knuckle component by tapping the steering knuckle.

## Wheel Hub, Steering Knuckle Component Installation Note

1. Apply grease (L2Y1 33247) to the wheel bearing inner race and drive shaft contact surface (Area A in figure).

2. Install the wheel hub, steering knuckle component.