#
REAR WHEEL ALIGNMENT

id021100800300

Rear wheel alignment specification (Unloaded*1)

Item | Fuel gauge indication
--- | ---
Empty | 1/4 | 1/2 | 3/4 | Full
Total toe-in | Tire [Tolerance ±4 {±0.16}] | (mm {in}) | 5 {0.2}
Rim inner | 3.0±2.4 {0.12±0.09} (14 inch wheel), 3.3±2.6 {0.13±0.10} (15 inch wheel)
(degree) | 0°28'±0°24'
Camber angle*2 (Reference value) [Tolerance ±1°] | -1°03' | -1°02'
Thrust angle [Tolerance ±0°48'] | 0° (Reference value)

  *1 :
Engine coolant and engine oil are at specified level. Spare tire, jack and tools are in designated position.
  *2 :
Difference between left and right must not exceed 1°30'.