#
DTC CONFIRMATION PROCEDURE

id010200618200

STEP | INSPECTION | ACTION
--- | --- | ---
1 | RECORD CONTINUOUS MEMORY DTC AND FREEZE FRAME DATA • Turn the ignition switch to the ON position (Engine off). • Connect the WDS or equivalent to the DLC-2. • Retrieve all stored DTCs. • Are any DTCs present? | Yes | Record all stored DTCs (Continuous Memory DTC) and Freeze Frame Data on the repair order, then go to the next step.
No | go to the next step.
2 | VERIFY RELATED SERVICE INFORMATION • Check for related Service Information availability. • Is any related Service Information available? | Yes | Perform repair or diagnosis according to the available Service Information. • If vehicle is not repaired, go to the next step.
No | Go to the next step.
3 | PERFORM SWITCH ON ENGINE OFF (KOEO) SELF-TEST • Start engine. • Warm up engine completely. • Turn off all electrical loads. • Perform the KOEO SELF-TEST PROCEDURE. (See KOEO/KOER SELF-TEST.) • Are any KOEO DTCs present? | Yes | Repair the KOEO DTC. (See DTC TABLE.)
No | Go to the next step.
4 | PERFORM SWITCH ON ENGINE RUNNING (KOER) SELF-TEST • Start engine. • Perform KOER SELF-TEST PROCEDURE. (See KOEO/KOER SELF-TEST.) • Are any KOER DTCs present? | Yes | Repair KOER DTC. (See DTC TABLE.)
No | • If any Continuous Memory DTC is present at Step 1, return to applicable the DTC troubleshooting procedure step. • If not Continuous Memory DTC is present at Step 1, go to symptom troubleshooting.