#
OIL FILTER REPLACEMENT [ZJ, ZY]

id011100800716

1. Remove the oil filter using the SST.

2. Use a clean rag to wipe off the mounting surface on the cylinder block.

3. Apply clean oil to a new O-ring of a new oil filter.

4. Remove the oil filter using the SST.

Tightening torque

  11.7-15.7 N·m {1.2-1.6 kgf·m, 8.7-11.5 ft·lbf}

5. Refill the engine with the type and amount of engine oil specified in the table.

6. Start the engine and inspect for oil leakage.

  • If the oil leaks, specify the faulty part and repair or replace it.

7. Inspect the oil level. (See ENGINE OIL LEVEL INSPECTION [ZJ, ZY].)