#
TRANSAXLE RANGE (TR) SWITCH CONSTRUCTION/OPERATION [FN4A-EL]

id0517a1109200
• A variable resistor type switch has been adopted for the transaxle range switch.
• Because the transaxle range switch and the selector lever are connected by the selector cable, the transaxle range switch indicates a certain resistance according to selector lever operation and from this the PCM determines the selector lever position. The corresponding signals are sent from the PCM to other related parts.