#
FRONT SEAT DISASSEMBLY/ASSEMBLY

id091300800300

## With Side Air Bag

  Warning

  • Handling the front seat (side air bag) improperly can accidentally deploy the side air bag, which may seriously injure you. Read AIR BAG SYSTEM SERVICE WARNINGS before handling the front seat. (See SERVICE WARNINGS.) (See SERVICE CAUTIONS.)

1. Disconnect the negative battery cable and wait for more than 1 minute.

2. Remove the side air bag module. (See SIDE AIR BAG MODULE REMOVAL/INSTALLATION.)

3. Disassemble in the order indicated in the table.

4. Assemble in the reverse order of disassembly.

1 | Headrest
2 | Recliner lever (lever type)
3 | Lifter lever
4 | Lifter lever cover
5 | Front buckle
6 | Side cover
7 | Reverse cover
8 | Rail cover
9 | Pole guide
10 | Seat back trim
11 | Seat back pad
12 | Seat back frame
13 | Seat cushion trim
14 | Seat cushion pad
15 | Seat cushion frame
16 | Slide adjuster

## Without Side Air Bag

1. Disassemble in the order indicated in the table.

2. Assemble in the reverse order of disassembly.

1 | Headrest
2 | Recliner lever (lever type)
3 | Lifter lever
4 | Lifter lever cover
5 | Front buckle
6 | Side cover
7 | Reverse cover
8 | Rail cover
9 | Pole guide
10 | Seat back trim
11 | Seat back pad
12 | Seat back frame
13 | Seat cushion trim
14 | Seat cushion pad
15 | Seat cushion frame
16 | Slide adjuster