#
TRANSMISSION/TRANSAXLE SPECIFICATIONS

id050000100600

## Clutch

Item | Specifications
--- | ---
Manual transaxle type | F35M-R
Clutch control | Hydraulic
Clutch cover | Spring type | Diaphragm
Set load | (N {kgf, lbf}) | 4,315 {440, 970}
Clutch disc | Outer diameter | (mm {in}) | 190 {7.48}
Inner diameter | (mm {in}) | 132 {5.20}
Clutch pedal | Type | Suspended
Pedal ratio | 5.54
Full stroke | (mm {in}) | 115 {4.53}
Clutch master cylinder inner diameter | (mm {in}) | 15.87 {0.625}
Clutch release cylinder inner diameter | (mm {in}) | 19.05 {0.750}
Clutch fluid type | SAE J1703, FMVSS116 DOT-3

## Manual Transaxle [F35M-R]

Item | Specifications
--- | ---
Engine type | ZJ, ZY
Transaxle type | F35M-R
Transaxle control | Floor-shift
Operation system | Cable
Shift assist | Forward | Synchromesh
Reverse | Selective sliding and synchromesh
Gear ratio | 1st | 3.416
2nd | 1.842
3rd | 1.290
4th | 0.972
5th | 0.775
Reverse | 3.214
Final gear ratio | 4.105
Oil | Grade | API service GL-4 or GL-5
Viscosity | All season | SAE 75W-90
Above 10 °C {50 °F} | SAE 80W-90
Capacity (approx. quantity) | (L {US qt, Imp qt}) | 3.04 {3.21, 2.68}

## Automatic Transaxle [FN4A-EL]

Item | Specifications
--- | ---
Engine type | ZY With WU-TWC | ZY Without WU-TWC
Transaxle type | FN4A-EL
Gear ratio | 1GR | 2.816
2GR | 1.497
3GR | 1.000
4GR | 0.725
Reverse | 2.648
Final gear ratio | 4.147
ATF | Type | ATF M-V
Capacity (approx. quantity) | (L {US qt, lmp qt}) | 7.0 {7.4, 6.2}
Torque converter stall torque ratio | 2.250
Hydraulic system | Forward clutch (number of drive/driven plates) | 4/4
3-4 clutch (number of drive/driven plates) | 3/3
Reverse clutch (number of drive/driven plates) | 2/2
Low and reverse brake (number of drive/driven plates) | 4/6 | 5/5
Band servo | Servo diameter (piston outer dia.) | (mm {in}) | 64.6 {2.54}
Front planetary gear (number of teeth) | Front sun gear | 49
Front pinion gear | 20
Front internal gear | 89
Rear planetary gear (number of teeth) | Rear sun gear | 37
Rear pinion gear | 30
Rear internal gear | 98
Primary gear | 86
Secondary gear | 82
Output gear | 20
Ring gear | 87