#
WHEEL APRON PANEL ASSEMBLY INSTALLATION

id098008614800

## LH

1. When installing new parts, position each part so that the section measurement aligns to the body dimension.

2. Drill holes for plug welds before installing new parts.

3. After trial-fitting new parts, make sure the related parts fit properly.

  Note

  • When replacing the wheel apron panel front and the suspension housing separately, weld 7 locations indicated by (A).

## RH

1. When installing new parts, position each part so that the section measurement aligns to the body dimension.

2. Drill holes for plug welds before installing new parts.

3. After trial-fitting new parts, make sure the related parts fit properly.

4. Install the bolt locations indicated by (A).

5. After installing, fillet weld in location (B).