#
DTC 07: ER07

id0902f6818200

DTC 07: Er07 | MD player
DETECTION CONDITION | Note • When error occurs, error message "CHECK MD" is displayed in the LCD. • Base unit detects MD reading error.
POSSIBLE CAUSE | • Defective MD (scratches or dirt) • MD player malfunction

Diagnostic procedure

Step | Inspection | Action
--- | --- | ---
1 | INSPECT MD • Inspect condition of MD where error has occurred. • Is MD okay? | Yes | Go to the next step.
No | Repair (remove foreign material) or replace MD, then go to the next step.
2 | INSPECT MD PLAYER • Clear DTC. • Insert and play MD for 12 s or more. • Start on-board diagnostic test mode. • Is DTC 07: Er07 displayed? | Yes | Replace MD player.
No | Troubleshooting completed.