PCM REMOVAL/INSTALLATION

id014000802400

  Note
  • When replacing the PCM, perform the following:
    ― PCM configuration (See PCM CONFIGURATION.)
    ― Immobilizer system-related part programming (See IMMOBILIZER SYSTEM COMPONENT REPLACEMENT/KEY ADDITION AND CLEARING.)
  • The PCM is integrated with the air cleaner cover and cannot be removed.

1. Remove the air cleaner cover. (See INTAKE-AIR SYSTEM REMOVAL/INSTALLATION [WITHOUT WU-TWC].)(See INTAKE-AIR SYSTEM REMOVAL/INSTALLATION [WITH WU-TWC].)