#
BRAKE SPECIFICATIONS

id040000100300

Item | Specification
--- | ---
Brake pedal | Type | Suspended
Pedal lever ratio | 3.79
Max. stroke | (mm {in}) | 136 {5.35}
Master cylinder | Type | Tandem (Plunger type)
Cylinder diameter | (mm {in}) | 23.81 {0.937}
Front brake (disc) | Type | Ventilated disc
Cylinder bore | (mm {in}) | 54.0 {2.13}
Pad dimensions (area × thickness) | 2,800 {4.34} × 12.5 {0.49}
(mm2 {in2} × mm {in})
Disc plate dimensions (outer diameter × thickness) | 258 {10.2} × 22.0 {0.87}
(mm {in})
Rear brake (drum) | Type | Leading-trailing
Wheel cylinder inner diameter | (mm {in}) | 19.05 {0.75}
Lining dimension (outer diameter × thickness) | (mm {in}) | 36.0 {1.42} × 163.0 {6.42} × 4.5 {0.18}
Drum inner diameter | (mm {in}) | 203 {7.99}
Shoe clearance adjustment | Automatic adjuster
Power brake unit | Type | Without ABS: Vacuum multiplier, single diaphragm With ABS: Vacuum multiplier, single diaphragm (With mechanical brake assist)
Diameter | (mm {in}) | 233.7 {9.20}
Braking force control device | Type | Without ABS: Proportioning valve With ABS: EBD (Electronic Brakeforce Distribution)
Parking brake | Type | Mechanical two-rear-wheel control
Operation system | Center lever type
Brake fluid | Type | SAE J1703, FMVSS116 DOT3