#
CYLINDER HEAD (II) DISASSEMBLY

id011000500500

1. Disassemble in the order indicated in the table.

1 | Valve keeper (See Valve Keeper Disassembly Note)
2 | Upper valve spring seat
3 | Valve spring
4 | Valve
5 | Valve seal (See Valve Seal Disassembly Note)

## Valve Keeper Disassembly Note

1. Remove the valve keeper using the SSTs.

## Valve Seal Disassembly Note

1. Remove the valve seal using the SST.