#
ENGINE FRONT COVER CONSTRUCTION [ZJ, ZY]

id0110001191b7
• The engine front cover is made of aluminum alloy, and is integrated with the No.3 engine mounting bracket to improve noise absorption and weight reduction.
• The service hole for unlocking the chain adjuster ratchet, and the service hole for securing the chain tensioner arm when loosening the timing chain tension are on the front cover for serviceability improvement.
• The installation hole for the oil control valve (OCV), the oil passage, and the oil filter are on the engine front cover. Oil filter maintenance is not necessary.
• The hole for installing the oil control valve (OCV) is provided.