#
WASHER TANK REMOVAL/INSTALLATION

id091900476100

1. Disconnect the negative battery cable.

2. Remove the front bumper. (See FRONT BUMPER REMOVAL/INSTALLATION.)

3. Remove the front combination light (LH). (See FRONT COMBINATION LIGHT REMOVAL/INSTALLATION.)

4. Remove in the order indicated in the table.

1 | Connector
2 | Washer hose (See Washer Hose Installation Note)
3 | Bolt
4 | Washer tank (See Washer Tank Removal Note)

5. Install in the reverse order of removal.

## Washer Tank Removal Note

1. Lift up the washer tank and remove the part a indicated in the figure from the shroud panel.

## Washer Hose Installation Note

1. Install the washer hoses placing them in the washer tank grooves.