#
DTC TABLE [FN4A-EL]

id0502a1800500
X: Available

DTC No. | Condition | MIL | HOLD indicator light flashes | DC | Monitor item | Memory function | Page
--- | --- | --- | --- | --- | --- | --- | ---
P0010 | CMP actuator circuit malfunction | (See DTC TABLE.)
P0011 | CMP timing over-advanced | (See DTC TABLE.)
P0012 | CMP timing over-retarded | (See DTC TABLE.)
P0031 | HO2S heater circuit low input | (See DTC TABLE.)
P0032 | HO2S heater circuit high input | (See DTC TABLE.)
P0102 | MAF circuit low input | (See DTC TABLE.)
P0103 | MAF circuit high input | (See DTC TABLE.)
P0112 | IAT circuit low input | (See DTC TABLE.)
P0113 | IAT circuit high input | (See DTC TABLE.)
P0117 | ECT circuit low input | (See DTC TABLE.)
P0118 | ECT circuit high input | (See DTC TABLE.)
P0122 | TP circuit low input | (See DTC TABLE.)
P0123 | TP circuit high input | (See DTC TABLE.)
P0131 | HO2S no inversion (stuck low) | (See DTC TABLE.)
P0132 | HO2S no inversion (stuck high) | (See DTC TABLE.)
P0134 | HO2S circuit no activity detected | (See DTC TABLE.)
P0171 | Fuel trim system too lean | (See DTC TABLE.)
P0172 | Fuel trim system too rich | (See DTC TABLE.)
P0327 | Knock sensor circuit low input | (See DTC TABLE.)
P0328 | Knock sensor circuit high input | (See DTC TABLE.)
P0335 | CKP sensor circuit malfunction | (See DTC TABLE.)
P0340 | CMP sensor circuit malfunction | (See DTC TABLE.)
P0351 | Ignition coil No.1 control circuit malfunction | (See DTC TABLE.)
P0352 | Ignition coil No.2 control circuit malfunction | (See DTC TABLE.)
P0353 | Ignition coil No.3 control circuit malfunction | (See DTC TABLE.)
P0354 | Ignition coil No.4 control circuit malfunction | (See DTC TABLE.)
P0443 | Evaporative emission control system purge control valve circuit malfunction | (See DTC TABLE.)
P0480 | Cooling fan relay No.1 control circuit malfunction | (See DTC TABLE.)
P0481 | Cooling fan relay No.2 control circuit malfunction | (See DTC TABLE.)
P0500 | Vehicle speed sensor (VSS) circuit malfunction (MTX) | (See DTC TABLE.)
Vehicle speed sensor (VSS) circuit malfunction (ATX) | ON | YES | 2 | CCM | X | (See DTC P0500 [FN4A-EL])
P0505 | Idle control system malfunction | (See DTC TABLE.)
P0511 | Idle control system circuit malfunction | (See DTC TABLE.)
P0537 | Evaporator temperature sensor circuit low input | (See DTC TABLE.)
P0538 | Evaporator temperature sensor circuit high input | (See DTC TABLE.)
P0602 | PCM programming error | (See DTC TABLE.)
P0610 | Control module vehicle options error | (See DTC TABLE.)
P0660 | VIS shutter valve actuator control circuit malfunction | (See DTC TABLE.)
P0668 | PCM temperature sensor circuit low input | (See DTC TABLE.)
P0669 | PCM temperature sensor circuit high input | (See DTC TABLE.)
P0706 | Transaxle range (TR) switch circuit range/performance | ON | YES | 2 | CCM | X | (See DTC P0706 [FN4A-EL])
P0707 | Transaxle range (TR) switch circuit low input | ON | YES | 1 | CCM | X | (See DTC P0707 [FN4A-EL])
P0708 | Transaxle range (TR) switch circuit high input | ON | YES | 2 | CCM | X | (See DTC P0708 [FN4A-EL])
P0711 | Transaxle fluid temperature (TFT) sensor circuit range/performance (Stuck) | ON | NO | 2 | CCM | X | (See DTC P0711 [FN4A-EL])
P0712 | Transaxle fluid temperature (TFT) sensor circuit malfunction (short to ground) | ON | YES | 1 | CCM | X | (See DTC P0712 [FN4A-EL])
P0713 | Transaxle fluid temperature (TFT) sensor circuit malfunction (open circuit) | ON | YES | 1 | CCM | X | (See DTC P0713 [FN4A-EL])
P0715 | Input/turbine speed sensor circuit malfunction | ON | YES | 1 | CCM | X | (See DTC P0715 [FN4A-EL])
P0731 | Gear 1 incorrect (incorrect gear ratio detected) | OFF | YES | 1 | CCM | X | (See DTC P0731 [FN4A-EL])
P0732 | Gear 2 incorrect (incorrect gear ratio detected) | OFF | YES | 1 | CCM | X | (See DTC P0732 [FN4A-EL])
P0733 | Gear 3 incorrect (incorrect gear ratio detected) | OFF | YES | 1 | CCM | X | (See DTC P0733 [FN4A-EL])
P0734 | Gear 4 incorrect (incorrect gear ratio detected) | OFF | YES | 1 | CCM | X | (See DTC P0734 [FN4A-EL])
P0741 | Torque converter clutch (TCC) (stuck OFF) | OFF | YES | 1 | CCM | X | (See DTC P0741 [FN4A-EL])
P0742 | Torque converter clutch (TCC) (stuck ON) | OFF | YES | 1 | CCM | X | (See DTC P0742 [FN4A-EL])
P0745 | Pressure control solenoid malfunction | OFF | YES | 1 | CCM | X | (See DTC P0745 [FN4A-EL])
P0751 | Shift solenoid A stuck OFF | ON | YES | 2 | CCM | X | (See DTC P0751 [FN4A-EL])
P0752 | Shift solenoid A stuck ON | ON | YES | 2 | CCM | X | (See DTC P0752 [FN4A-EL])
P0753 | Shift solenoid A malfunction (electrical) | ON | YES | 1 | CCM | X | (See DTC P0753 [FN4A-EL])
P0756 | Shift solenoid B stuck OFF | ON | YES | 2 | CCM | X | (See DTC P0756 [FN4A-EL])
P0757 | Shift solenoid B stuck ON | ON | YES | 2 | CCM | X | (See DTC P0757 [FN4A-EL])
P0758 | Shift solenoid B malfunction (electrical) | ON | YES | 1 | CCM | X | (See DTC P0758 [FN4A-EL])
P0761 | Shift solenoid C stuck OFF | ON | YES | 2 | CCM | X | (See DTC P0761 [FN4A-EL])
P0762 | Shift solenoid C stuck ON | ON | YES | 2 | CCM | X | (See DTC P0762 [FN4A-EL])
P0763 | Shift solenoid C malfunction (electrical) | ON | YES | 1 | CCM | X | (See DTC P0763 [FN4A-EL])
P0766 | Shift solenoid D stuck OFF | ON | YES | 2 | CCM | X | (See DTC P0766 [FN4A-EL])
P0767 | Shift solenoid D stuck ON | ON | YES | 2 | CCM | X | (See DTC P0767 [FN4A-EL])
P0768 | Shift solenoid D malfunction (electrical) | ON | YES | 1 | CCM | X | (See DTC P0768 [FN4A-EL])
P0771 | Shift solenoid E stuck OFF | ON | YES | 2 | CCM | X | (See DTC P0771 [FN4A-EL])
P0772 | Shift solenoid E stuck ON | ON | YES | 2 | CCM | X | (See DTC P0772 [FN4A-EL])
P0773 | Shift solenoid E malfunction (electrical) | ON | YES | 1 | CCM | X | (See DTC P0773 [FN4A-EL])
P1384 | Variable valve timing control system malfunction | (See DTC TABLE.)
P1562 | PCM +BB voltage low | (See DTC TABLE.)
P2008 | VTCS shutter valve actuator control circuit malfunction | (See DTC TABLE.)
P2502 | Generator terminal B circuit open | (See DTC TABLE.)
P2503 | Generator output voltage signal no electricity | (See DTC TABLE.)
P2504 | Battery overcharge | (See DTC TABLE.)
U0073 | CAN bus off | (See DTC TABLE [MULTIPLEX COMMUNICATION SYSTEM])
U0121 | PCM cannot receive any signals from ABS, ABS/TCS or DSC HU/CM | (See DTC TABLE [MULTIPLEX COMMUNICATION SYSTEM])
U0155 | PCM cannot receive any signals from combination meter | (See DTC TABLE [MULTIPLEX COMMUNICATION SYSTEM])