#
SELECTOR CABLE ADJUSTMENT

id051800271600

1. Remove the center console.

2. Shift the selector lever to P position.

3. Unlock the lock piece of the selector cable (selector lever side) in the order shown in the figure.

4. Verify that the manual shaft is in P position.

5. Lock the lock piece of the selector cable (selector lever side) in the order shown in the figure.

6. Install the center console.

7. Shift the selector lever from P position to L range, and make sure that there are no other components in that area to interfere with the lever.