#
DTC B1342

id0802a0801100

DTC B1342 | SAS control module (air bag system warning light DTC 12 is displayed.)
--- | ---
SAS control module DTC 12 detection circuit malfunction (the air bag system warning light illuminates continuously.)
DETECTION CONDITION | Warning • Detection conditions are for understanding the DTC outline before performing an inspection. Performing an inspection with only detection conditions may cause injury due to an operating error, or damage the system. When performing an inspection, always follow the inspection procedure. • When the SAS control module internal circuit has a malfunction.
POSSIBLE CAUSE | • SAS control module malfunction

Diagnostic procedure

Action
Replace the SAS control module. (See SAS CONTROL MODULE REMOVAL/INSTALLATION.)