#
WASHER MOTOR INSPECTION

id091900477200

1. Connect battery positive voltage to the motor terminal A and ground to the motor terminal B.

2. Verify that the washer fluid flows through the windshield washer hose.

  • If there is any malfunction, replace the washer motor.

3. Connect battery positive voltage to the motor terminal B and ground to the motor terminal A. (with rear wiper)

4. Verify that the washer fluid flows through the rear washer hose.

  • If there is any malfunction, replace the washer motor.