#
BONNET ADJUSTMENT

id091000407300

## Gap Adjustment

1. Verify that the gap between the bonnet and the body is within the specification.

Clearance

  a: 4.0-7.0 mm {0.16-0.27 in}
  b: 2.7-4.7 mm {0.11-0.18 in}

2. Remove the front fender panel.

3. Loosen the bonnet hinge installation bolts and reposition the bonnet hinges.

4. Tighten the bolts.

5. Install the front fender panel.

## Height Difference Adjustment

1. Turn the stop rubber to adjust the height of the bonnet.

2. Verify that the height difference between the bonnet and the body is within the specification.

Clearance

  a: 4.0-8.0 mm {0.16-0.31 in}
  b: -0.9-3.1 mm {-0.035-0.12 in}
  c: -1.5-0.5 mm {-0.59-0.019 in}