#
DTC 00: ER03

id0902f6816900

DTC 00: Er03 | Cassette deck
DETECTION CONDITION | • Base unit detects that reel built into cassette deck does not operate.
POSSIBLE CAUSE | • Defective cassette tape (tape slack, pinched tape in internal cassette deck) • Cassette deck malfunction

Diagnostic procedure

Step | Inspection | Action
--- | --- | ---
1 | INSPECT CASSETTE TAPE • Inspect condition of cassette tape where error has occurred. • Is cassette tape okay? | Yes | Go to the next step.
No | Repair (remove tape slack or repair pinched tape) or replace cassette tape, then go to the next step.
2 | INSPECT CASSETTE DECK • Clear DTC. • Insert cassette tape with no defect. • Play cassette tape for 20 s or more. • Start on-board diagnostic test mode. • Is DTC 00: Er03 displayed? | Yes | Replace cassette deck.
No | Troubleshooting completed.