#
PRE-DELIVERY INSPECTION

id000000801100

## PRE-DELIVERY INSPECTION TABLE

### EXTERIOR

• INSPECT and ADJUST, if necessary, the following items to specification:

□Glass, exterior bright metal and paint for damage

□All weatherstrips for damage or detachment

□Door operation and alignment including side door and back door

□Wheel lug nuts

□Tire pressures

□Headlight aiming

□Operation of bonnet release and lock

□Operation of liftgate and fuel-filler lid opener

• INSTALL the following parts:

□Flap (front and rear)

□Wheel caps or rings (if equipped)

### UNDER BONNET-ENGINE OFF

• INSPECT and ADJUST, if necessary, the following items to specification:

□Fuel, engine coolant, and hydraulic lines, fittings, connections, and components for leaks

□Accelerator cable and linkage for free movement

□Tightness of water hose clamps

□Tightness of battery terminals, electrolyte level and specific gravity

□Radiator coolant level and specific gravity

□Engine oil level

□Oil level in steering gearbox

□Windshield washer tank fluid level

□Brake master cylinder fluid level

□Clutch master cylinder fluid level

□Power steering fluid level

□Manual transaxle oil level

CLEAN the spark plugs

### INTERIOR

• INSTALL the following parts:

□Fuse for accessories

• CHECK the operations of the following items:

□All lights including warning, and indicator lights

□Cigarette lighter and clock

□Ignition switch and steering lock

□Transaxle range switch

□Warning buzzers

□Ignition key reminder alarm

□Seat controls (sliding and reclining) and headrests

□Seat belts warning system

□Door locks, including childproof door locks

□Power door lock

□Power windows (if equipped)

□Horn, wipers, and washers

□Wiper blades performance

Clean the wiper blades and windshield, if necessary

□Antenna

• CHECK the following items:

□Presence of spare fuse

□Upholstery and interior finish

• CHECK and ADJUST, if necessary, the following items:

□Operation and fit of windows

□Parking brake

□Pedal height and free play of brake pedal

### UNDER BONNET-ENGINE RUNNING AT OPERATING TEMPERATURE

  • CHECK the following items:

□Operation of idle-up system for electrical load, air conditioner

□Idle speed

□Automatic transaxle fluid level

□Initial ignition timing

□Operation of throttle position sensor

□Operation of EGR valve

### ON HOIST

  • CHECK the following items:

□Underside fuel, coolant and hydraulic lines, fittings, connections, and components for leaks

□Tires for cuts or bruises

□Steering linkage, suspension, exhaust system, and all underside hardware for looseness or damage

### ROAD TEST

• CHECK the following items:

□Brake operation

□Clutch operation

□Steering control

□Operation of meters and gauges, squeaks, rattles, and abnormal noises

□Engine general performance

□Emergency locking retractors

### AFTER ROAD TEST

• REMOVE the seat and floor mat protective covers

CHECK for the necessary owner information materials, tools, and spare tire in vehicle