#
INTERLOCK CABLE ADJUSTMENT

id051800800300

1. Pull up the lock piece of the interlock cable to release the lock.

2. Remove the clip of the selector lever base plate, remove the interlock cable from the U-groove.

3. Remove the interlock cable from the selector lever.

4. Fully pull the end of the interlock cable to selector lever.

5. Push the slider pin to the stopper plate and rotate to lock.

6. Push the snap pin (or a ø1.5 round bar or similar) into hole A by fully pushing in the slider pin.

7. Push the snap pin into hole B and hole C of the lock unit until it passes through.

8. Fully push the end of the interlock cable to the selector lever.

9. Lock the lock piece of the interlock cable.