#
AUTOMATIC TRANSAXLE FEATURES

id051700101800

Realization of excellent shift quality | • Electronic pressure-adjusting control of line pressure by a liner type solenoid (pressure control solenoid) adopted • Electronic control (direct electric shift control) of clutch pressure by duty-cycle type solenoids (shift solenoid A, B, and C) adopted • Centrifugal balance clutch chamber adopted
High efficiency, compactness, and light weight | • Miniature trochoid gear type oil pump with torque converter direct drive adopted • Bonded seal piston adopted • Tow-step final gear drive mechanism adopted
Improved reliability, reduced NVH (noise, vibration and harshness) | • Double arranged gears with a single planetary gear unit adopted