TRANSMISSION/TRANSAXLE TECHNICAL DATA

id055000800100

Clutch

Item | Specification
--- | ---
Clutch fluid type | SAE J1703, FMVSS 116 DOT-3
Clutch pedal height | 303 mm {11.9 in}
Clutch pedal free play | 15 mm {0.59 in} or less
Clutch pedal disengagement stroke | 80—100 mm {3.2—3.9 in}
Clutch cover diaphragm spring fingers maximum depth | 0.6 mm {0.024 in}
Maximum clearance of flatness of the pressure plate | 0.5 mm {0.020 in}
Clutch cover diaphragm spring fingers maximum misalignment | 1.0 mm {0.039 in}
Clutch disc minimum thickness | 0.3 mm {0.012 in}
Clutch disc maximum runout | 0.7 mm {0.028 in}
Flywheel maximum runout | 0.13 mm {0.0051 in}

Manual Transaxle

Item | Specification
--- | ---
Manual transaxle oil | Grade: API Service GL-4 or GL-5 Viscosity (all-season): SAE 75W-90 Viscosity (above 10 °C {50 °F}): SAE 80W-90 Capacity (approx. quantity): 3.04 L {3.21 US qt, 2.68 lmp qt}

Automatic Transaxle

Item | Specification
--- | ---
Time lag | N position → D range: 0.4—0.7 s N position → R position: 0.4—0.7 s
ATF | Type: ATF M‐V Capacity (approx. quantity): 7.0 L {7.4 US qt, 6.1 lmp qt}
Input/turbine speed sensor resistance | 250—600 ohms (ATF temperature: –40—160 °C {–40—320 °F})
Vehicle speedometer sensor (VSS) voltage | 4.5—5.5 V

Line pressure

Position/Range | Specification (kPa {kgf/cm2, psi})
--- | ---
D, S, L (Includes each HOLD mode) | Idle | 330—470 {3.4—4.7, 48—68}
Stall | 1,030—1,190 {10.5—12.1, 150—172}
R | Idle | 490—710 {5.0—7.2, 71—102}
Stall | 1,700—2,050 {17.4—20.9, 247—297}

Engine stall speed

Position/Range | Specification (rpm)
--- | ---
D, S, L (Includes each HOLD mode) | 2,000—2,600
R

Transaxle range (TR) switch

Terminal | Position/Range | Resistance (ohm)
--- | --- | ---
B—C | P | 4,085—4,515
R | 1,425—1,575
N | 713—788
D | 371—410
S | 190—210
L | 87—96

Transaxle fluid temperature (TFT) sensor

ATF temperature (°C {°F}) | Resistance (kilohm)
--- | ---
–20 {–4} | 236—324
0 {32} | 84.3—110.0
20 {68} | 33.5—42.0
40 {104} | 14.7—17.9
60 {140} | 7.08—8.17
80 {176} | 3.61—4.15
100 {212} | 1.96—2.24
120 {248} | 1.13—1.28
130 {266} | 0.87—0.98

Solenoid valve resistance (ATF temperature: –40—150 °C {–40—302 °F})

Terminal | Solenoid valve | Resistance (ohm)
--- | --- | ---
A—GND | Shift solenoid A | 1.0—4.2
C—GND | Shift solenoid B | 1.0—4.2
G—GND | Shift solenoid C | 1.0—4.2
B—GND | Shift solenoid D | 10.9—26.2
F—GND | Shift solenoid E | 10.9—26.2
D—I | Pressure control | 2.4—7.3