POWER BRAKE UNIT REMOVAL/INSTALLATION

id041100801800

  Caution
  • Once the brake switch clearance has automatically been adjusted, it cannot be adjusted again. Therefore, replace the switch with a new one when replacing the power brake unit or performing any procedure that changes the pedal stroke.

1. Remove the master cylinder. (See MASTER CYLINDER REMOVAL/INSTALLATION.)

2. Remove in the order indicated in the table.

am2zzw00006714

1 | Vacuum hose
2 | Joint pin (See BRAKE PEDAL REMOVAL/INSTALLATION.)
3 | Nut
4 | Power brake unit

3. Remove the brake switch. (See BRAKE PEDAL REMOVAL/INSTALLATION.)

4. Install in the reverse order of removal.

5. After installation, inspect the shift-lock and key interlock.