#
INTERIOR LIGHT CONTROL SYSTEM OPERATION

id091800526000
• The interior light switch must be at DOOR position.

Condition before operation (When all conditions are satisfied) | Operation condition | Interior light | Cancel condition (When any condition is satisfied)
Illumination time | Brightness
• Ignition switch at LOCK or ACC position. (IG off.) • All doors are closed. (All door switches are off.) | Any door is open. (Any door switch is on.) | Approx. 5 minutes | 100% | • All doors are closed. (All door switches are off.) • After illumination time.*
• Key extracted from steering lock. (Key reminder switch is off.) • All doors are closed. (All door switches are off.) • Driver's door lock knob is locked. (Door lock-link switch is in lock position.) | Driver's door lock knob is unlocked. (Door lock-link switch is in unlock position.) | Approx. 30 seconds | 100% | • Ignition switch at ON position. (IG on.) • Any door is open. (Any door switch is on.) • Driver's door lock knob is locked. (Door lock-link switch is in lock position.) • After illumination time.*
• Key inserted into steering lock. (Key reminder switch is on.) • All doors are closed. (All door switches are off.) | Key extracted from steering lock. (Key reminder switch is off.) | Approx. 15 seconds | 100% | • Ignition switch at ON position. (IG on.) • Any door is open. (Any door switch is on.) • Driver's door lock knob is locked. (Door lock-link switch is in lock position.) • After illumination time.*
• Ignition switch at LOCK or ACC position. (IG off.) • Any door is open. (Any door switch is on.) • Driver's door lock knob is unlocked. (Door lock-link switch is in unlock position.) | All doors are closed. (All door switches are off.) | Approx. 15 seconds | 60% | • Ignition switch at ON position. (IG on.) • Any door is open. (Any door switch is on.) • Driver's door lock knob is locked. (Door lock-link switch is in lock position.) • After illumination time.*

  * :
After interior light is turned off according to this cancel condition, the light will illuminate again when either of the following conditions are satisfied.

• After all doors are closed, then any door is reopened. (After all door switches are off, any door switch is on.)
• Ignition switch is at ON position. (IG on.)

## Timing Chart