#
ENGINE DISASSEMBLY/ASSEMBLY [ZJ, ZY]

id0110008005b7

1. Using the bolts part number 99794 1025 or M10×1.25, length 25 mm {0.98 in} to install the SST to the position shown in the figure, hang the engine and transaxle, and then take it down from the engine jack.

Tightening torque

  38-51 N·m {3.9-5.2 kgf·m, 29-37 ft·lbf}

2. Remove the engine from the transaxle. (See MANUAL TRANSAXLE REMOVAL/INSTALLATION [F35M-R].) (See AUTOMATIC TRANSAXLE REMOVAL/INSTALLATION [FN4A-EL].)

3. Remove the EGR pipe and EGR valve bracket. (With EGR) (See INTAKE-AIR SYSTEM REMOVAL/INSTALLATION [WITH WU-TWC].) (See EXHAUST SYSTEM REMOVAL/INSTALLATION [WITH WU-TWC].) (See EGR VALVE REMOVAL/INSTALLATION [WITH WU-TWC].)

4. Remove the intake-air system. (See INTAKE-AIR SYSTEM REMOVAL/INSTALLATION [WITHOUT WU-TWC].) (See INTAKE-AIR SYSTEM REMOVAL/INSTALLATION [WITH WU-TWC].)

5. Remove the exhaust system. (See EXHAUST SYSTEM REMOVAL/INSTALLATION [WITHOUT WU-TWC].) (See EXHAUST SYSTEM REMOVAL/INSTALLATION [WITH WU-TWC].)

6. Remove the generator. (See GENERATOR REMOVAL/INSTALLATION [ZJ, ZY].)

7. Remove the P/S oil pump. (See POWER STEERING OIL PUMP REMOVAL/INSTALLATION.)

8. Remove the ignition coil. (See IGNITION COIL REMOVAL/INSTALLATION [ZJ, ZY].)

9. Remove the crankshaft position (CKP) sensor. (See CRANKSHAFT POSITION (CKP) SENSOR REMOVAL/INSTALLATION.)

10. Install in the reverse order of removal.